FS = "\t";
HEADER = 1;
RECCNT = OFF;
MTXCNT_OUT = 1;
MATCNT_OUT = 1;
ORD_IGNORE = 0;

{
	UINT id; 
	UINT level?; 
	UINT var_of_level?; 
	ASCF effect1_desc; 
	ASCF effect2_desc; 
	ASCF effect3_desc?; 
}

/*
	Originally submitted by
	czardadius

	remark from me: last entry is a gamble -
	- may be char, may be ascf, etc.
*/
